# STRING FORMAT OF IF RECEIVER CONTROL CARD

**$,Att3,Att1,Att2,Ps1,Ps2,Ps3,#**

* Att1:-Attenuator1 value (0-31.5 (0.5 Resolution))
* Att2:- Attenuator2 value (0-31.5 (0.5 Resolution))
* Att3:- Attenuator2 value (0-31.5 (0.5 Resolution))
* Ps1:-Dac1 Voltage (0 to 15 (0.1Resolution))
* Ps2:- Dac2 Voltage (0 to 15 (0.1Resolution))
* Ps3:- Dac3 Voltage (0 to 15 (0.1Resolution))